[Device]
Family=ecp5u
PartType=LFE5U-25F
PartName=LFE5U-25F-6BG381C
SpeedGrade=6
Package=CABGA381
OperatingCondition=COM
Status=S

[IP]
VendorName=Lattice Semiconductor Corporation
CoreType=LPM
CoreStatus=Demo
CoreName=RAM_DP_TRUE
CoreRevision=7.5
ModuleName=sr_font
SourceFormat=verilog
ParameterFileVersion=1.0
Date=09/19/2017
Time=16:11:47

[Parameters]
Verilog=1
VHDL=0
EDIF=1
Destination=Synplicity
Expression=BusA(0 to 7)
Order=Big Endian [MSB:LSB]
IO=0
RAddress=4096
RData=8
WAddress=4096
WData=8
ROutputEn=0
RClockEn=0
WOutputEn=0
WClockEn=0
enByte=0
ByteSize=9
Optimization=Speed
Reset=Sync
Reset1=Sync
Init=mem
MemFile=e:/work/lattice/ohm/next186_soc/font.mem
MemFormat=hex
EnECC=0
Pipeline=0
WriteA=Normal
WriteB=Normal
init_data=0

[FilesGenerated]
e:/work/lattice/ohm/next186_soc/font.mem=mem

[Command]
cmd_line= -w -n sr_font -lang verilog -synth synplify -bus_exp 7 -bb -arch sa5p00 -type ramdp -device LFE5U-25F -aaddr_width 12 -widtha 8 -baddr_width 12 -widthb 8 -anum_words 4096 -bnum_words 4096 -cascade -1 -memfile e:/work/lattice/ohm/next186_soc/font.mem -memformat hex -writemodeA NORMAL -writemodeB NORMAL
