(edif dcm1
  (edifVersion 2 0 0)
  (edifLevel 0)
  (keywordMap (keywordLevel 0))
  (status
    (written
      (timestamp 2016 9 26 11 40 13)
      (program "SCUBA" (version "Diamond (64-bit) 3.5.1.302"))))
      (comment "C:\lscc\diamond\3.5_x64\ispfpga\bin\nt64\scuba.exe -w -n dcm1 -lang verilog -synth synplify -arch xo2c00 -type pll -fin 50 -fclkop 29.4912 -fclkop_tol 2.0 -fclkos 11.289600 -fclkos_tol 1.0 -trimp 0 -phasep 0 -trimp_r -trims 0 -phases 0 -trims_r -phase_cntl STATIC -fb_mode 1 ")
  (library ORCLIB
    (edifLevel 0)
    (technology
      (numberDefinition))
    (cell VLO
      (cellType GENERIC)
      (view view1
        (viewType NETLIST)
        (interface
          (port Z
            (direction OUTPUT)))))
    (cell EHXPLLJ
      (cellType GENERIC)
      (view view1
        (viewType NETLIST)
        (interface
          (port CLKI
            (direction INPUT))
          (port CLKFB
            (direction INPUT))
          (port PHASESEL1
            (direction INPUT))
          (port PHASESEL0
            (direction INPUT))
          (port PHASEDIR
            (direction INPUT))
          (port PHASESTEP
            (direction INPUT))
          (port LOADREG
            (direction INPUT))
          (port STDBY
            (direction INPUT))
          (port PLLWAKESYNC
            (direction INPUT))
          (port RST
            (direction INPUT))
          (port RESETM
            (direction INPUT))
          (port RESETC
            (direction INPUT))
          (port RESETD
            (direction INPUT))
          (port ENCLKOP
            (direction INPUT))
          (port ENCLKOS
            (direction INPUT))
          (port ENCLKOS2
            (direction INPUT))
          (port ENCLKOS3
            (direction INPUT))
          (port PLLCLK
            (direction INPUT))
          (port PLLRST
            (direction INPUT))
          (port PLLSTB
            (direction INPUT))
          (port PLLWE
            (direction INPUT))
          (port PLLADDR4
            (direction INPUT))
          (port PLLADDR3
            (direction INPUT))
          (port PLLADDR2
            (direction INPUT))
          (port PLLADDR1
            (direction INPUT))
          (port PLLADDR0
            (direction INPUT))
          (port PLLDATI7
            (direction INPUT))
          (port PLLDATI6
            (direction INPUT))
          (port PLLDATI5
            (direction INPUT))
          (port PLLDATI4
            (direction INPUT))
          (port PLLDATI3
            (direction INPUT))
          (port PLLDATI2
            (direction INPUT))
          (port PLLDATI1
            (direction INPUT))
          (port PLLDATI0
            (direction INPUT))
          (port CLKOP
            (direction OUTPUT))
          (port CLKOS
            (direction OUTPUT))
          (port CLKOS2
            (direction OUTPUT))
          (port CLKOS3
            (direction OUTPUT))
          (port LOCK
            (direction OUTPUT))
          (port INTLOCK
            (direction OUTPUT))
          (port REFCLK
            (direction OUTPUT))
          (port CLKINTFB
            (direction OUTPUT))
          (port DPHSRC
            (direction OUTPUT))
          (port PLLACK
            (direction OUTPUT))
          (port PLLDATO7
            (direction OUTPUT))
          (port PLLDATO6
            (direction OUTPUT))
          (port PLLDATO5
            (direction OUTPUT))
          (port PLLDATO4
            (direction OUTPUT))
          (port PLLDATO3
            (direction OUTPUT))
          (port PLLDATO2
            (direction OUTPUT))
          (port PLLDATO1
            (direction OUTPUT))
          (port PLLDATO0
            (direction OUTPUT)))))
    (cell dcm1
      (cellType GENERIC)
      (view view1
        (viewType NETLIST)
        (interface
          (port CLKI
            (direction INPUT))
          (port CLKOP
            (direction OUTPUT))
          (port CLKOS
            (direction OUTPUT)))
        (property NGD_DRC_MASK (integer 1))
        (contents
          (instance scuba_vlo_inst
            (viewRef view1 
              (cellRef VLO)))
          (instance PLLInst_0
            (viewRef view1 
              (cellRef EHXPLLJ))
            (property DDRST_ENA
              (string "DISABLED"))
            (property DCRST_ENA
              (string "DISABLED"))
            (property MRST_ENA
              (string "DISABLED"))
            (property PLLRST_ENA
              (string "DISABLED"))
            (property INTFB_WAKE
              (string "DISABLED"))
            (property STDBY_ENABLE
              (string "DISABLED"))
            (property DPHASE_SOURCE
              (string "DISABLED"))
            (property PLL_USE_WB
              (string "DISABLED"))
            (property CLKOS3_FPHASE
              (string "0"))
            (property CLKOS3_CPHASE
              (string "0"))
            (property CLKOS2_FPHASE
              (string "0"))
            (property CLKOS2_CPHASE
              (string "0"))
            (property CLKOS_FPHASE
              (string "0"))
            (property CLKOS_CPHASE
              (string "47"))
            (property CLKOP_FPHASE
              (string "0"))
            (property CLKOP_CPHASE
              (string "17"))
            (property PLL_LOCK_MODE
              (string "0"))
            (property CLKOS_TRIM_DELAY
              (string "0"))
            (property CLKOS_TRIM_POL
              (string "RISING"))
            (property CLKOP_TRIM_DELAY
              (string "0"))
            (property CLKOP_TRIM_POL
              (string "RISING"))
            (property FRACN_DIV
              (string "0"))
            (property FRACN_ENABLE
              (string "DISABLED"))
            (property OUTDIVIDER_MUXD2
              (string "DIVD"))
            (property PREDIVIDER_MUXD1
              (string "0"))
            (property VCO_BYPASS_D0
              (string "DISABLED"))
            (property CLKOS3_ENABLE
              (string "DISABLED"))
            (property OUTDIVIDER_MUXC2
              (string "DIVC"))
            (property PREDIVIDER_MUXC1
              (string "0"))
            (property VCO_BYPASS_C0
              (string "DISABLED"))
            (property CLKOS2_ENABLE
              (string "DISABLED"))
            (property FREQUENCY_PIN_CLKOS
              (string "11.250000"))
            (property OUTDIVIDER_MUXB2
              (string "DIVB"))
            (property PREDIVIDER_MUXB1
              (string "0"))
            (property VCO_BYPASS_B0
              (string "DISABLED"))
            (property CLKOS_ENABLE
              (string "ENABLED"))
            (property FREQUENCY_PIN_CLKOP
              (string "30.000000"))
            (property OUTDIVIDER_MUXA2
              (string "DIVA"))
            (property PREDIVIDER_MUXA1
              (string "0"))
            (property VCO_BYPASS_A0
              (string "DISABLED"))
            (property CLKOP_ENABLE
              (string "ENABLED"))
            (property FREQUENCY_PIN_CLKI
              (string "50.000000"))
            (property ICP_CURRENT
              (string "8"))
            (property LPF_RESISTOR
              (string "8"))
            (property CLKOS3_DIV
              (string "1"))
            (property CLKOS2_DIV
              (string "1"))
            (property CLKOS_DIV
              (string "48"))
            (property CLKOP_DIV
              (string "18"))
            (property CLKFB_DIV
              (string "3"))
            (property CLKI_DIV
              (string "5"))
            (property FEEDBK_PATH
              (string "CLKOP")))
          (net LOCK
            (joined
              (portRef LOCK (instanceRef PLLInst_0))))
          (net scuba_vlo
            (joined
              (portRef Z (instanceRef scuba_vlo_inst))
              (portRef PLLADDR4 (instanceRef PLLInst_0))
              (portRef PLLADDR3 (instanceRef PLLInst_0))
              (portRef PLLADDR2 (instanceRef PLLInst_0))
              (portRef PLLADDR1 (instanceRef PLLInst_0))
              (portRef PLLADDR0 (instanceRef PLLInst_0))
              (portRef PLLDATI7 (instanceRef PLLInst_0))
              (portRef PLLDATI6 (instanceRef PLLInst_0))
              (portRef PLLDATI5 (instanceRef PLLInst_0))
              (portRef PLLDATI4 (instanceRef PLLInst_0))
              (portRef PLLDATI3 (instanceRef PLLInst_0))
              (portRef PLLDATI2 (instanceRef PLLInst_0))
              (portRef PLLDATI1 (instanceRef PLLInst_0))
              (portRef PLLDATI0 (instanceRef PLLInst_0))
              (portRef PLLWE (instanceRef PLLInst_0))
              (portRef PLLSTB (instanceRef PLLInst_0))
              (portRef PLLRST (instanceRef PLLInst_0))
              (portRef PLLCLK (instanceRef PLLInst_0))
              (portRef ENCLKOS3 (instanceRef PLLInst_0))
              (portRef ENCLKOS2 (instanceRef PLLInst_0))
              (portRef ENCLKOS (instanceRef PLLInst_0))
              (portRef ENCLKOP (instanceRef PLLInst_0))
              (portRef RESETD (instanceRef PLLInst_0))
              (portRef RESETC (instanceRef PLLInst_0))
              (portRef RESETM (instanceRef PLLInst_0))
              (portRef RST (instanceRef PLLInst_0))
              (portRef PLLWAKESYNC (instanceRef PLLInst_0))
              (portRef STDBY (instanceRef PLLInst_0))
              (portRef LOADREG (instanceRef PLLInst_0))
              (portRef PHASESTEP (instanceRef PLLInst_0))
              (portRef PHASEDIR (instanceRef PLLInst_0))
              (portRef PHASESEL1 (instanceRef PLLInst_0))
              (portRef PHASESEL0 (instanceRef PLLInst_0))))
          (net CLKOS
            (joined
              (portRef CLKOS)
              (portRef CLKOS (instanceRef PLLInst_0))))
          (net CLKOP
            (joined
              (portRef CLKOP)
              (portRef CLKFB (instanceRef PLLInst_0))
              (portRef CLKOP (instanceRef PLLInst_0))))
          (net CLKI
            (joined
              (portRef CLKI)
              (portRef CLKI (instanceRef PLLInst_0))))))))
  (design dcm1
    (cellRef dcm1
      (libraryRef ORCLIB)))
)
